**H8–E24**

**SPECIFICATION GUIDELINES**

The framed installation for the suspended ceiling will be created using PLAFOMETAL H8-E15 metal panels made from **\* steel** in dimensions of **\* dimensions** and a height of 7.5 mm. PLAFOMETAL will adapt the thickness according to the required dimensions.

Metal tiles will be **\*non-perforated / perforated** and equipped with an additional acoustic component: **\*acoustic**

**Installation**

The ceiling will be installed on a PLAFOMETAL T24 grid system.

A channel trim of the same color as the grid will ensure the peripheral finish at the level of the walls and partition walls.

The metal tiles will rest on the grid, creating a 24 x 8 hollow joint for installation on a T24.

The grid will be fully exposed.

The product will be fitted in accordance with the requirements of the local code of practice. For specific applications, users must contact PLAFOMETAL to ensure that the technical characteristics are suitable for the intended use.

**\* Insert your choice in the drop-down list of colors**

